MCLAUGHLIN WASTE EQUIPMENT INC.
FLATBED ROLL OFF BODY
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Standard Specifications
· 12’ to 24’ Long
· 7 GA. Floor Diamond Plate 12” to Ground
· 4’ Headboard w/Expanded Metal Window
· 6”x2”x1/4” Tubing Main Rails or 6” Channel 
· 3” Channel Crossmembers on 16” Centers
· Basic Hook Up Options Included (A-Frame Extra)
· 8”x8” Boogie Wheels or Stands 12” Floor Height
· 96” Wide Deck (Fits Most Tarping Systems) 
· Rub Rail & Stack Pockets (3” Channel)
· Painted Black or White
· Underseal Under Floor
Options 
· Front Push Plate ¼” & Stack Holders
· Winches Fixed or Sliding
· Sloped Rear Ramp
· D-Rings With & With Out Recess
· Flat Steel or Other Gauges
· Recess Wheels 10” to Ground
· 102” Wide Deck
· Choice of Paint Colors
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